**PAT-TRAP® SERIAL NUMBER LOCATION**



The Serial Number is stamped on the edge of the ¼” steel plate.

**Measurements of the Pat-Trap machine**

From the bottom of the base to the top of the King Pin 24”

From the bottom of the base to the top of the turret 34 ¾ “

Trap cog top max – 39 ½ ”

Trap cog bottom min – 37”

Wobble base to throw plate (up/down angles) min 17 ¾”

Wobble base to throw plate (up/down angles) max 24 ½ “

Wobble max – 39 ½ “

Wobble Min – 34 ¾ “

Diagram 4

notch

A fully crated Pat-Trap is 500 #.

Machine and pump weighs 350 #.

Turret weigh 50 #.

Pump weight 50 #.

Pat-Trap machine w/o pump and turret weight 250 #.

Pallet Dimensions are 46X38X38

43”

**Base Dimensions of PAT-TRAP®**



**Serial Number is stamped here.**

**Example: “G4190”**

**Also located on pump.**

Diagram 5

**PAT-TRAP® Serial Number Location**

Serial Number Location: The Serial Number is stamped on the front left edge (shooting stand 1 Side) of the ¼” thick steel “Throw Plate”.